RTF65002 Reference Guide

2013

robfinch@finitron.ca

Finitron

1/1/2013

# RTF65002

Table of Contents

[RTF65002 1](#_Toc369128888)

[General Registers 6](#_Toc369128889)

[Special Purpose Registers 6](#_Toc369128890)

[Addressing Modes 7](#_Toc369128891)

[Memory Addressing 7](#_Toc369128892)

[Vectors 8](#_Toc369128893)

[Native mode vector table: 8](#_Toc369128894)

[Instruction Set Summary 9](#_Toc369128895)

[ADD 9](#_Toc369128896)

[SUB 10](#_Toc369128897)

[CMP 10](#_Toc369128898)

[AND 11](#_Toc369128899)

[BIT 11](#_Toc369128900)

[OR 12](#_Toc369128901)

[ORB 12](#_Toc369128902)

[EOR 12](#_Toc369128903)

[Load and Store Instructions 13](#_Toc369128904)

[LD 13](#_Toc369128905)

[LB 13](#_Toc369128906)

[LDA 13](#_Toc369128907)

[LDX 13](#_Toc369128908)

[LDY 14](#_Toc369128909)

[ST 15](#_Toc369128910)

[SB 15](#_Toc369128911)

[STA 15](#_Toc369128912)

[STX 16](#_Toc369128913)

[STY 16](#_Toc369128914)

[STZ 16](#_Toc369128915)

[Shift Operations / Read-modify-write memory operations. 17](#_Toc369128916)

[ASL 17](#_Toc369128917)

[ROL 17](#_Toc369128918)

[LSR 17](#_Toc369128919)

[ROR 17](#_Toc369128920)

[INC 18](#_Toc369128921)

[DEC 18](#_Toc369128922)

[Bitmap Instructions 19](#_Toc369128923)

[BMS 19](#_Toc369128924)

[BMC 19](#_Toc369128925)

[BMF 19](#_Toc369128926)

[BMT 19](#_Toc369128927)

[LDX 20](#_Toc369128928)

[STX 20](#_Toc369128929)

[CPX 20](#_Toc369128930)

[INX 20](#_Toc369128931)

[DEX 20](#_Toc369128932)

[PHX 20](#_Toc369128933)

[PLX 20](#_Toc369128934)

[LDY 20](#_Toc369128935)

[STY 20](#_Toc369128936)

[CPY 20](#_Toc369128937)

[INY 21](#_Toc369128938)

[DEY 21](#_Toc369128939)

[PHY 21](#_Toc369128940)

[PLY 21](#_Toc369128941)

[Flow Control 22](#_Toc369128942)

[JMP 22](#_Toc369128943)

[JSR 22](#_Toc369128944)

[RTS 22](#_Toc369128945)

[RTI 22](#_Toc369128946)

[BRA 23](#_Toc369128947)

[BEQ 23](#_Toc369128948)

[BNE 23](#_Toc369128949)

[BPL 23](#_Toc369128950)

[BMI 23](#_Toc369128951)

[BVS 23](#_Toc369128952)

[BVC 23](#_Toc369128953)

[BCS 23](#_Toc369128954)

[BCC 23](#_Toc369128955)

[BHI 23](#_Toc369128956)

[BLS 23](#_Toc369128957)

[BLT 23](#_Toc369128958)

[BLE 23](#_Toc369128959)

[BGT 23](#_Toc369128960)

[BGE 23](#_Toc369128961)

[BEQ 23](#_Toc369128962)

[BNE 23](#_Toc369128963)

[BPL 23](#_Toc369128964)

[BMI 23](#_Toc369128965)

[BVS 23](#_Toc369128966)

[BVC 23](#_Toc369128967)

[BCS 23](#_Toc369128968)

[BCC 23](#_Toc369128969)

[BRL 23](#_Toc369128970)

[BSR 24](#_Toc369128971)

[BRK 24](#_Toc369128972)

[NOP 24](#_Toc369128973)

[WAI 24](#_Toc369128974)

[STP 24](#_Toc369128975)

[Stack push and pop operations. 25](#_Toc369128976)

[PHP 25](#_Toc369128977)

[PHA 25](#_Toc369128978)

[PHX 25](#_Toc369128979)

[PHY 25](#_Toc369128980)

[PUSH 25](#_Toc369128981)

[PUSHA 25](#_Toc369128982)

[PLP 25](#_Toc369128983)

[PLA 25](#_Toc369128984)

[PLX 25](#_Toc369128985)

[PLY 25](#_Toc369128986)

[POP 25](#_Toc369128987)

[POPA 25](#_Toc369128988)

[CLC 25](#_Toc369128989)

[SEC 25](#_Toc369128990)

[CLV 25](#_Toc369128991)

[CLI 25](#_Toc369128992)

[SEI 25](#_Toc369128993)

[CLD 25](#_Toc369128994)

[SED 25](#_Toc369128995)

[EMM 25](#_Toc369128996)

[Register to register transfer short forms. 26](#_Toc369128997)

[TAX 26](#_Toc369128998)

[TXA 26](#_Toc369128999)

[TAY 26](#_Toc369129000)

[TYA 26](#_Toc369129001)

[TAS 26](#_Toc369129002)

[TSA 26](#_Toc369129003)

[TYX 26](#_Toc369129004)

[TXY 26](#_Toc369129005)

[TSX 26](#_Toc369129006)

[TXS 26](#_Toc369129007)

[TRS 26](#_Toc369129008)

[TSR 26](#_Toc369129009)

[EXEC 26](#_Toc369129010)

[ATNI 26](#_Toc369129011)

[String Operations 27](#_Toc369129012)

[MVN 27](#_Toc369129013)

[MVP 27](#_Toc369129014)

[STOS 27](#_Toc369129015)

[CMPS 27](#_Toc369129016)

## General Registers

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | Usage |
| R0 |  | This register is always zero |  |
| R1 | acc | Accumulator | First parameter / return value |
| R2 | x | ‘x’ index register | Second parameter / Loop counter |
| R3 | y | ‘y’ index register | Third parameter |
| R4 |  |  |  |
| R5 |  |  |  |
| R6 |  |  |  |
| R7 |  |  |  |
| R8 |  |  |  |
| R9 |  |  |  |
| R10 |  |  |  |
| R11 |  |  |  |
| R12 |  |  |  |
| R13 |  |  |  |
| R14 |  |  |  |
| R15 |  |  |  |
|  |  |  |  |

## Special Purpose Registers

|  |  |  |  |
| --- | --- | --- | --- |
| Code |  |  |  |
| 0 | cc | Cache control register |  |
|  | ice | Bit 0 = instruction cache enable | |
| dce | Bit 1 = Data cache enable | |
| dcwa | Bit 2 = Data cache write allocate policy (1=allocate) | |
| … |  |  |  |
| 3 | ph | Multiplier product high order 32 bits | |
| 4 | tick | Tick counter | Read only |
| 5 | lfsr | Linear feedback shift register | Pseudo random |
| … |  |  | |
| 8 | vbr | Vector base register – the lower 9 bits are always zero  Bit 0 = interrupt policy (1=native mode for all external interrupts) | |
| 14 | sp8 | 8 bit mode stack pointer | Upper 24 bits set the stack page |
| 15 | sp | Native mode Stack pointer |  |
|  |  |  |  |

## Addressing Modes

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | Clock Cycles |  |
| Rn | Register direct | 2 |  |
| #imm8 | Eight bit sign extended immediate | 2 |  |
| #imm16 | Sixteen bit sign extended immediate | 2 |  |
| #imm32 | Thirty-two bit immediate | 2 |  |
| zp,Rb | Zero page indexed | 4 |  |
| (zp,Rb) | Zero page indexed indirect (inner indexed) | 5 |  |
| (zp),Rb | Zero page indirect indexed (outer indexed) | 6 |  |
| abs | absolute | 4 |  |
| abs,Rb | Absolute indexed | 4 |  |
| (Rb) | Register indirect | 4 |  |
| Label | Relative branch | 2 |  |

## Memory Addressing

The cpu is word oriented for data and byte oriented for code. Up to 4GW of data are supported and 4GB of code.

The byte load/store instructions can address only the lower 4GB of the address space.

Index registers automatically scale to the data size. Incrementing a register used as an index moves to the next word if word size data is being processed (the norm) or to the next byte if byte sized data is being processed (lb/sb).

# Vectors

The processor vectors through $0FFFFFFF8 on a reset, and $0FFFFFFF4 on a non-maskable interrupt. In 32 bit mode, or with native mode on interrupt set, all other vectoring is done through a vector table. The vector table allows for 512 entries. The vector table base address is established by the VBR register. During an external IRQ the processor looks at a vector number bus to determine the vector to use for the IRQ. This vector number may be hard-coded in which case all IRQ’s will be vectored to the same location.

In eight bit mode the IRQ/BRK vectors through the usual eight bit IRQ vector at $0FFFE.

### Native mode vector table:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Vector Number | Usage / Description | |  |  |
| 0 | BREAK instruction vector | |  |  |
| 1 | SLEEP vector (branch to self) | |  |  |
| 2 | Task reschedule interrupt | |  |  |
| … |  | |  |  |
| 448 | Spurious interrupt | |  |  |
| 449 | IRQ level 1 | 1000 Hz interrupt |  |  |
| 450 | IRQ level 2 | 100 Hz interrupt |  |  |
| … | Other IRQ levels |  |  |  |
| 463 | IRQ level 15 | keyboard interrupt |  |  |
| … |  | |  |  |
| 495 | Unimplemented instruction | |  |  |
| … |  | |  |  |
| 508 | Bus error – data load / store | |  |  |
| 509 | Bus error – instruction fetch | |  |  |
| 511 |  | |  |  |

# Instruction Set Summary

The cycle counts are assuming no wait states are required for either instructions or data and both instructions and data can be found in the cache.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ADD | | Flags: v c n z | | | | | | | | | Bytes | Cyc |
| Byte 7 | Byte 6 | | Byte5 | Byte 4 | Byte 3 | | Byte 2 | | Byte 1 |  |  |  |
|  | | | | | 0 | Rt | Rb | Ra | 02h | ADD Rt,Ra,Rb | 3 | 2 |
|  | | | | | Imm8 | | Rt | Ra | 65h | ADD Rt,Ra,#imm8 | 3 | 2 |
|  | | | | Imm16 | | | Rt | Ra | 79h | ADD Rt,Ra,#imm16 | 4 | 2 |
|  | | Imm32 | | | | | Rt | Ra | 69h | ADD Rt,Ra,#imm32 | 6 | 2 |
|  | | | | Addr12 | | Rt | Rb | Ra | 75h | ADD Rt,Ra,zp,Rb | 4 | 4 |
|  | | | | Addr12 | | Rt | Rb | Ra | 61h | ADD Rt,Ra,(zp,Rb) | 4 | 5 |
|  | | | | Addr12 | | Rt | Rb | Ra | 71h | ADD Rt,Ra,(zp),Rb | 4 | 6 |
|  | | Addr32 | | | | | Rt | Ra | 6Dh | ADD Rt,Ra,abs | 6 | 4 |
| Addr32 | | | | | ~4 | Rt | Rb | Ra | 7Dh | ADD Rt,Ra,abs,Rb | 7 | 4 |
|  | | | | | ~4 | Rt | Rb | Ra | 72h | ADD Rt,Ra,(Rb) | 3 | 4 |
|  | | | | | Disp8 | | Rt | Ra | 63h | ADD Rt,Ra,d,sp | 3 | 4 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SUB | Flags: v c n z | | | | | | | | | | | | Bytes | Cyc |
|  | |  | | | 1 | | | Rt | Rb | Ra | 02h | SUB Rt,Ra,Rb | 3 | 2 |
|  | |  |  | | | Imm8 | | | Rt | Ra | E5h | SUB Rt,Ra,#imm8 | 3 | 2 |
|  | |  | Imm16 | | | | | | Rt | Ra | F9h | SUB Rt,Ra,#imm16 | 4 | 2 |
|  | Imm32 | | | | | | | | Rt | Ra | E9h | SUB Rt,Ra,#imm32 | 6 | 2 |
|  | |  | Addr12 | | | | Rt | | Rb | Ra | F5h | SUB Rt,Ra,zp,Rb | 4 | 4 |
|  | |  | Addr12 | | | | Rt | | Rb | Ra | E1h | SUB Rt,Ra, (zp,Rb) | 4 | 5 |
|  | |  | Addr12 | | | | Rt | | Rb | Ra | F1h | SUB Rt,Ra, (zp),Rb | 4 | 6 |
|  | Addr32 | | | | | | | | Rt | Ra | EDh | SUB Rt,Ra,abs | 6 | 4 |
| Addr32 | | | | | |  | Rt | | Rb | Ra | FDh | SUB Rt,Ra,abs,Rb | 7 | 4 |
|  | | | | | ~4 | | | Rt | Rb | Ra | F2h | SUB Rt,Ra, (Rb) | 3 | 4 |
|  | | | | Disp8 | | | | | Rt | Ra | E3h | SUB Rt,Ra,d,sp | 3 | 4 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| CMP | Flags: c n z | | | | | | | | | | | | Bytes | |
|  | |  | | 1 | | | 0 | Rb | Ra | | 02h | CMP Ra,Rb | 3 | |
|  | |  |  | | Imm8 | | | 0 | Ra | | E5h | CMP Ra,#imm8 | 3 | |
|  | |  | Imm16 | | | | | 0 | Ra | | F9h | CMP Ra,#imm16 | 4 | |
|  | Imm32 | | | | | | | 0 | Ra | | E9h | CMP Ra,#imm32 | 6 | |
|  | |  | Addr12 | | | 0 | | Rb | Ra | | F5h | CMP Ra,zp,Rb | 4 | |
|  | |  | Addr12 | | | 0 | | Rb | Ra | | E1h | CMP Ra, (zp,Rb) | 4 | |
|  | |  | Addr12 | | | 0 | | Rb | Ra | | F1h | CMP Ra, (zp),Rb | 4 | |
|  | Addr32 | | | | | | | 0 | Ra | | EDh | CMP Ra,abs | 6 | |
| Addr32 | | | | |  | 0 | | Rb | Ra | | FDh | CMP Ra,abs,Rb | 7 | |
|  | | | | ~4 | | | 0 | Rb | Ra | | F2h | CMP Ra, (Rb) | 3 | |
|  | | | | | Disp8 | | | 0 | | Ra | E3h | CMP Ra,d,sp | 3 |  |
|  | | | | | | | | Imm8 | | | C5h | CMP #imm8 | 2 | |

CMP is an alternate mnemonic for SUB where the target register is R0. CMP does not affect the overflow flag.

* Opcode C5h compares the accumulator to a sign extended eight bit value.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| AND | Flags: n z | | | | | | | | | | | | Bytes |
|  | |  | | 3 | | | Rt | Rb | Ra | | 02h | AND Rt,Ra,Rb | 3 |
|  | |  |  | | Imm8 | | | Rt | Ra | | 25h | AND Rt,Ra,#imm8 | 3 |
|  | |  | Imm16 | | | | | Rt | Ra | | 39h | AND Rt,Ra,#imm16 | 4 |
|  | Imm32 | | | | | | | Rt | Ra | | 29h | AND Rt,Ra,#imm32 | 6 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 35h | AND Rt,Ra,zp,Rb | 4 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 21h | AND Rt,Ra, (zp,Rb) | 4 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 31h | AND Rt,Ra, (zp),Rb | 4 |
|  | Addr32 | | | | | | | Rt | Ra | | 2Dh | AND Rt,Ra,abs | 6 |
| Addr32 | | | | |  | Rt | | Rb | Ra | | 3Dh | AND Rt,Ra,abs,Rb | 7 |
|  | | | | ~4 | | | Rt | Rb | Ra | | 32h | AND Rt,Ra, (Rb) | 3 |
|  | | | | | Disp8 | | | Rt | | Ra | 23h | AND Rt,Ra,d,sp | 3 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| BIT | Flags: v n z | | | | | | | | | | | | Bytes |
|  | |  | | 3 | | | 0 | Rb | Ra | | 02h | BIT Ra,Rb | 3 |
|  | |  |  | | Imm8 | | | 0 | Ra | | 25h | BIT Ra,#imm8 | 3 |
|  | |  | Imm16 | | | | | 0 | Ra | | 39h | BIT Ra,#imm16 | 4 |
|  | Imm32 | | | | | | | 0 | Ra | | 29h | BIT Ra,#imm32 | 6 |
|  | |  | Addr12 | | | 0 | | Rb | Ra | | 35h | BIT Ra,zp,Rb | 4 |
|  | |  | Addr12 | | | 0 | | Rb | Ra | | 21h | BIT Ra, (zp,Rb) | 4 |
|  | |  | Addr12 | | | 0 | | Rb | Ra | | 31h | BIT Ra, (zp),Rb | 4 |
|  | Addr32 | | | | | | | 0 | Ra | | 2Dh | BIT Ra,abs | 6 |
| Addr32 | | | | |  | 0 | | Rb | Ra | | 3Dh | BIT Ra,abs,Rb | 7 |
|  | | | | ~4 | | | 0 | Rb | Ra | | 32h | BIT Ra, (Rb) | 3 |
|  | | | | | Disp8 | | | Rt | | Ra | 23h | BIT Ra,d,sp | 3 |

Bit is the AND operation with no target register; the overflow status is set to bit 30 of the memory op

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| OR | Flags: n z | | | | | | | | | | | | Bytes |
|  | |  | | 5 | | | Rt | Rb | Ra | | 02h | OR Rt,Ra,Rb | 3 |
|  | |  |  | | Imm8 | | | Rt | Ra | | 05h | OR Rt,Ra,#imm8 | 3 |
|  | |  | Imm16 | | | | | Rt | Ra | | 19h | OR Rt,Ra,#imm16 | 4 |
|  | Imm32 | | | | | | | Rt | Ra | | 09h | OR Rt,Ra,#imm32 | 6 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 15h | OR Rt,Ra,zp,Rb | 4 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 01h | OR Rt,Ra, (zp,Rb) | 4 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 11h | OR Rt,Ra, (zp),Rb | 4 |
|  | Addr32 | | | | | | | Rt | Ra | | 0Dh | OR Rt,Ra,abs | 6 |
| Addr32 | | | | |  | Rt | | Rb | Ra | | 1Dh | OR Rt,Ra,abs,Rb | 7 |
|  | | | | ~4 | | | Rt | Rb | Ra | | 12h | OR Rt,Ra, (Rb) | 3 |
|  | | | | | Disp8 | | | Rt | | Ra | 03h | OR Rt,Ra,d,sp | 3 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ORB | Flags: n z | | | | | | | | | Bytes |
|  | |  | Addr12 | | Rt | Rb | Ra | B5h | OR Rt,Ra,zp,Rb | 4 |
|  | Addr32 | | | | | Rt | Ra | ADh | OR Rt,Ra,abs | 6 |
| Addr32 | | | |  | Rt | Rb | Ra | BDh | OR Rt,Ra,abs,Rb | 7 |

The ORB instruction loads a byte from memory and zero extends it before performing an OR operation. The address fields represent a byte address.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| EOR | Flags: n z | | | | | | | | | | | | Bytes |
|  | |  | | 4 | | | Rt | Rb | Ra | | 02h | EOR Rt,Ra,Rb | 3 |
|  | |  |  | | Imm8 | | | Rt | Ra | | 45h | EOR Rt,Ra,#imm8 | 3 |
|  | |  | Imm16 | | | | | Rt | Ra | | 59h | EOR Rt,Ra,#imm16 | 4 |
|  | Imm32 | | | | | | | Rt | Ra | | 49h | EOR Rt,Ra,#imm32 | 6 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 55h | EOR Rt,Ra,zp,Rb | 4 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 41h | EOR Rt,Ra, (zp,Rb) | 4 |
|  | |  | Addr12 | | | Rt | | Rb | Ra | | 51h | EOR Rt,Ra, (zp),Rb | 4 |
|  | Addr32 | | | | | | | Rt | Ra | | 4Dh | EOR Rt,Ra,abs | 6 |
| Addr32 | | | | |  | Rt | | Rb | Ra | | 5Dh | EOR Rt,Ra,abs,Rb | 7 |
|  | | | | ~4 | | | Rt | Rb | Ra | | 52h | EOR Rt,Ra, (Rb) | 3 |
|  | | | | | Disp8 | | | Rt | | Ra | 43h | EOR Rt,Ra,d,sp | 3 |

## Load and Store Instructions

Arithmetic and logical instructions can take a memory operand as the third operand of the instruction. This effectively turns all these instructions into load instructions. Hence there isn’t an explicit load instruction. The OR or EOR instructions can readily be used to perform a load operation.

Because addresses are word addresses, the address field in the instructions is normally shifted left twice resulting in a 34 bit data address. The only exception to this is the byte load and store instructions.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LD | Flags: n z | | | | | | | | | | | | Bytes |
|  | |  |  | | Imm8 | | | Rt | 0 | | 05h | LD Rt,#imm8 | 3 |
|  | |  | Imm16 | | | | | Rt | 0 | | 19h | LD Rt,#imm16 | 4 |
|  | Imm32 | | | | | | | Rt | 0 | | 09h | LD Rt,#imm32 | 6 |
|  | |  | Addr12 | | | Rt | | Rb | 0 | | 15h | LD Rt,zp,Rb | 4 |
|  | |  | Addr12 | | | Rt | | Rb | 0 | | 01h | LD Rt, (zp,Rb) | 4 |
|  | |  | Addr12 | | | Rt | | Rb | 0 | | 11h | LD Rt, (zp),Rb | 4 |
|  | Addr32 | | | | | | | Rt | 0 | | 0Dh | LD Rt,abs | 6 |
| Addr32 | | | | |  | Rt | | Rb | 0 | | 1Dh | LD Rt,abs,Rb | 7 |
|  | | | | ~4 | | | Rt | Rb | 0 | | 12h | LD Rt, (Rb) | 3 |
|  | | | | | Disp8 | | | Rt | | 0 | 03h | LD Rt,Ra,d,sp | 3 |
|  | | | | | | | | Rt | Ra | | 7Bh | LD Rt,Ra | 2 |

LD is an alternate mnemonic for the OR instruction where register Ra is zero.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LB | Flags: n z | | | | | | | | | Bytes |
|  | |  | Addr12 | | Rt | Rb | Ra | B5h | LB Rt,Ra,zp,Rb | 4 |
|  | Addr32 | | | | | Rt | Ra | ADh | LB Rt,Ra,abs | 6 |
| Addr32 | | | |  | Rt | Rb | Ra | BDh | LB Rt,Ra,abs,Rb | 7 |

LB is an alternate mnemonic for the ORB instruction where register Ra is zero.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LDA | Flags: n z | | | | | | | | | | | | Bytes |
|  | |  |  | | Imm8 | | | 1 | 0 | | 05h | LDA #imm8 | 3 |
|  | |  | Imm16 | | | | | 1 | 0 | | 19h | LDA #imm16 | 4 |
|  | Imm32 | | | | | | | 1 | 0 | | 09h | LDA #imm32 | 6 |
|  | |  | Addr12 | | | 1 | | Rb | 0 | | 15h | LDA zp,Rb | 4 |
|  | |  | Addr12 | | | 1 | | Rb | 0 | | 01h | LDA (zp,Rb) | 4 |
|  | |  | Addr12 | | | 1 | | Rb | 0 | | 11h | LDA (zp),Rb | 4 |
|  | Addr32 | | | | | | | Rt | 0 | | 0Dh | LDA abs | 6 |
| Addr32 | | | | |  | 1 | | Rb | 0 | | 1Dh | LDA abs,Rb | 7 |
|  | | | | ~4 | | | 1 | Rb | 0 | | 12h | LDA (Rb) | 3 |
|  | | | | | Disp8 | | | 1 | | 0 | 03h | LDA d,sp | 3 |

LDA is an alternate mnemonic for the OR instruction where register Ra is zero and register Rt is one.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LDX | Flags: n z | | | | | | | | | | | Bytes |
|  | |  |  | | Imm8 | | | 2 | 0 | 05h | LDX #imm8 | 3 |
|  | |  | Imm16 | | | | | 2 | 0 | 19h | LDX #imm16 | 4 |
|  | Imm32 | | | | | | | 2 | 0 | 09h | LDX #imm32 | 6 |
|  | |  | Addr12 | | | 2 | | Rb | 0 | 15h | LDX zp,Rb | 4 |
|  | |  | Addr12 | | | 2 | | Rb | 0 | 01h | LDX (zp,Rb) | 4 |
|  | |  | Addr12 | | | 2 | | Rb | 0 | 11h | LDX (zp),Rb | 4 |
|  | Addr32 | | | | | | | Rt | 0 | 0Dh | LDX abs | 6 |
| Addr32 | | | | |  | 2 | | Rb | 0 | 1Dh | LDX abs,Rb | 7 |
|  | | | | ~4 | | | 2 | Rb | 0 | 12h | LDX (Rb) | 3 |

LDX is an alternate mnemonic for the OR instruction where register Ra is zero and register Rt is two.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LDY | Flags: n z | | | | | | | | | | | Bytes |
|  | |  |  | | Imm8 | | | 3 | 0 | 05h | LDY #imm8 | 3 |
|  | |  | Imm16 | | | | | 3 | 0 | 19h | LDY #imm16 | 4 |
|  | Imm32 | | | | | | | 3 | 0 | 09h | LDY #imm32 | 6 |
|  | |  | Addr12 | | | 3 | | Rb | 0 | 15h | LDY zp,Rb | 4 |
|  | |  | Addr12 | | | 3 | | Rb | 0 | 01h | LDY (zp,Rb) | 4 |
|  | |  | Addr12 | | | 3 | | Rb | 0 | 11h | LDY (zp),Rb | 4 |
|  | Addr32 | | | | | | | Rt | 0 | 0Dh | LDY abs | 6 |
| Addr32 | | | | |  | 3 | | Rb | 0 | 1Dh | LDY abs,Rb | 7 |
|  | | | | ~4 | | | 3 | Rb | 0 | 12h | LDY (Rb) | 3 |

LDY is an alternate mnemonic for the OR instruction where register Ra is zero and register Rt is three.

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ST | Flags: none | | | | | | | | | | Bytes |
|  | |  | Addr12 | | 0 | Rb | Ra | | 95h | ST Ra,zp,Rb | 4 |
|  | |  | Addr12 | | 0 | Rb | Ra | | 81h | ST Ra, (zp,Rb) | 4 |
|  | |  | Addr12 | | 0 | Rb | Ra | | 91h | ST Ra, (zp),Rb | 4 |
|  | Addr32 | | | | | 0 | Ra | | 8Dh | ST Ra,abs | 6 |
| Addr32 | | | |  | 0 | Rb | Ra | | 9Dh | ST Ra,abs,Rb | 7 |
|  | | | | | | Rb | Ra | | 92h | ST Ra, (Rb) | 2 |
|  | | | | Disp8 | | 0 | | Ra | 83h | ST Ra,d,sp | 3 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SB | Flags: none | | | | | | | | | Bytes |
|  | |  | Addr12 | | 0 | Rb | Ra | 74h | SB Ra,zp,Rb | 4 |
|  | Addr32 | | | | | 0 | Ra | 9Ch | SB Ra,abs | 6 |
| Addr32 | | | |  | 0 | Rb | Ra | 9Eh | SB Ra,abs,Rb | 7 |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| STA | Flags: none | | | | | | | | | | Bytes |
|  | |  | Addr12 | | 0 | Rb | 1 | | 95h | STA zp,Rb | 4 |
|  | |  | Addr12 | | 0 | Rb | 1 | | 81h | STA (zp,Rb) | 4 |
|  | |  | Addr12 | | 0 | Rb | 1 | | 91h | STA (zp),Rb | 4 |
|  | Addr32 | | | | | 0 | 1 | | 8Dh | STA abs | 6 |
| Addr32 | | | |  | 0 | Rb | 1 | | 9Dh | STA abs,Rb | 7 |
|  | | | | | | Rb | 1 | | 92h | STA (Rb) | 2 |
|  | | | | Disp8 | | 0 | | 1 | 83h | STA Ra,d,sp | 3 |

STA is an alternate mnemonic for ST where the register to be stored is R1 (the accumulator).

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| STX | Flags: none | | | | | | | | | | Bytes |
|  | |  | Addr12 | | 0 | Rb | 2 | | 95h | STX zp,Rb | 4 |
|  | |  | Addr12 | | 0 | Rb | 2 | | 81h | STX (zp,Rb) | 4 |
|  | |  | Addr12 | | 0 | Rb | 2 | | 91h | STX (zp),Rb | 4 |
|  | Addr32 | | | | | 0 | 2 | | 8Dh | STX abs | 6 |
| Addr32 | | | |  | 0 | Rb | 2 | | 9Dh | STX abs,Rb | 7 |
|  | | | | | | Rb | 2 | | 92h | STX (Rb) | 2 |
|  | | | | Disp8 | | 0 | | 2 | 83h | STX d,sp | 3 |

STX is an alternate mnemonic for ST where the register to be stored is R2 (the x index register). There are also additional short-hand forms for the STX instruction.

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| STY | Flags: none | | | | | | | | | | Bytes |
|  | |  | Addr12 | | 0 | Rb | 3 | | 95h | STY zp,Rb | 4 |
|  | |  | Addr12 | | 0 | Rb | 3 | | 81h | STY (zp,Rb) | 4 |
|  | |  | Addr12 | | 0 | Rb | 3 | | 91h | STY (zp),Rb | 4 |
|  | Addr32 | | | | | 0 | 3 | | 8Dh | STY abs | 6 |
| Addr32 | | | |  | 0 | Rb | 3 | | 9Dh | STY abs,Rb | 7 |
|  | | | | | | Rb | 3 | | 92h | STY (Rb) | 2 |
|  | | | | Disp8 | | 0 | | 3 | 83h | STY d,sp | 3 |

STY is an alternate mnemonic for ST where the register to be stored is R3 (the y index register). There are also additional short-hand forms for the STY instruction.

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| STZ | Flags: none | | | | | | | | | | Bytes |
|  | |  | Addr12 | | 0 | Rb | 0 | | 95h | STZ zp,Rb | 4 |
|  | |  | Addr12 | | 0 | Rb | 0 | | 81h | STZ (zp,Rb) | 4 |
|  | |  | Addr12 | | 0 | Rb | 0 | | 91h | STZ (zp),Rb | 4 |
|  | Addr32 | | | | | 0 | 0 | | 8Dh | STZ abs | 6 |
| Addr32 | | | |  | 0 | Rb | 0 | | 9Dh | STZ abs,Rb | 7 |
|  | | | | | | Rb | 0 | | 92h | STZ (Rb) | 2 |
|  | | | | Disp8 | | 0 | | 0 | 83h | STZ d,sp | 3 |

STZ is an alternate mnemonic for ST where the register to be stored is R0.

## Shift Operations / Read-modify-write memory operations.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ASL | Flags: c n z | | | | | | | | | | | Bytes |
|  | |  | |  | | | |  |  | 0Ah | ASL acc | 1 |
|  | |  | |  | | | | Rt | Ra | 06h | ASL Rt,Ra | 2 |
|  | |  | |  | Addr12 | | | | Rb | 16h | ASL zp,Rb | 3 |
|  |  | | Addr32 | | | | | | | 0Eh | ASL abs | 5 |
|  | Addr32 | | | | | | | Rb | 0 | 1Eh | ASL abs,Rb | 6 |
|  |  | | | | Eh | | Rt | Rb | Ra | 02h | ASL Rt,Ra,Rb | 3 |
|  |  | | | | ~3 | Imm5 | | Rt | Ra | 24h | ASL Rt,Ra,#imm8 | 3 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ROL | Flags: c n z | | | | | | | | | Bytes |
|  | |  | |  | |  |  | 2Ah | ROL acc | 1 |
|  | |  | |  | | Rt | Ra | 26h | ROL Rt,Ra | 2 |
|  | |  | |  | Addr12 | | Rb | 36h | ROL zp,Rb | 3 |
|  |  | | Addr32 | | | | | 2Eh | ROL abs | 5 |
|  | Addr32 | | | | | Rb | 0 | 3Eh | ROL abs,Rb | 6 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LSR | Flags: c n z | | | | | | | | | | | Bytes |
|  | |  | |  | | | |  |  | 4Ah | LSR acc | 1 |
|  | |  | |  | | | | Rt | Ra | 46h | LSR Rt,Ra | 2 |
|  | |  | |  | Addr12 | | | | Rb | 56h | LSR zp,Rb | 3 |
|  |  | | Addr32 | | | | | | | 4Eh | LSR abs | 5 |
|  | Addr32 | | | | | | | Rb | 0 | 5Eh | LSR abs,Rb | 6 |
|  |  | | | | Fh | | Rt | Rb | Ra | 02h | LSR Rt,Ra,Rb | 3 |
|  |  | | | | ~3 | Imm5 | | Rt | Ra | 34h | LSR Rt,Ra,#imm8 | 3 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ROR | Flags: c n z | | | | | | | | | Bytes |
|  | |  | |  | |  |  | 6Ah | ROR acc | 1 |
|  | |  | |  | | Rt | Ra | 66h | ROR Rt,Ra | 2 |
|  | |  | |  | Addr12 | | Rb | 76h | ROR zp,Rb | 3 |
|  |  | | Addr32 | | | | | 6Eh | ROR abs | 5 |
|  | Addr32 | | | | | Rb | 0 | 7Eh | ROR abs,Rb | 6 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| INC | Flags: n z | | | | | | | | | Bytes |
|  | |  | |  | |  |  |  |  |  |
|  | |  | |  | | Rt | Ra | E6h | INC Rt,Ra | 2 |
|  | |  | |  | Addr12 | | Rb | F6h | INC zp,Rb | 3 |
|  |  | | Addr32 | | | | | EEh | INC abs | 5 |
|  | Addr32 | | | | | Rb | 0 | FEh | INC abs,Rb | 6 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DEC | Flags: n z | | | | | | | | | Bytes |
|  | |  | |  | |  |  |  |  |  |
|  | |  | |  | | Rt | Ra | C6h | DEC Rt,Ra | 2 |
|  | |  | |  | Addr12 | | Rb | D6h | DEC zp,Rb | 3 |
|  |  | | Addr32 | | | | | CEh | DEC abs | 5 |
|  | Addr32 | | | | | Rb | 0 | DEh | DEC abs,Rb | 6 |

## Bitmap Instructions

The bitmap instructions take a bit number in the accumulator and combine it with the address supplied in the instruction in order to set,clear,flip or test a bit in memory.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| BMS | Flags: | | | | | | | | | Bytes |
|  | |  | |  | Addr12 | | Rb | 0642h | BMS zp,Rb | 4 |
|  |  | | Addr32 | | | | | 0E42h | BMS abs | 6 |
|  | Addr32 | | | | | Rb | 0 | 1E42h | BMS abs,Rb | 7 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| BMC | Flags: | | | | | | | | | Bytes |
|  | |  | |  | Addr12 | | Rb | 2642h | BMS zp,Rb | 4 |
|  |  | | Addr32 | | | | | 2E42h | BMS abs | 6 |
|  | Addr32 | | | | | Rb | 0 | 3E42h | BMS abs,Rb | 7 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| BMF | Flags: | | | | | | | | | Bytes |
|  | |  | |  | Addr12 | | Rb | 4642h | BMS zp,Rb | 4 |
|  |  | | Addr32 | | | | | 4E42h | BMS abs | 6 |
|  | Addr32 | | | | | Rb | 0 | 5E42h | BMS abs,Rb | 7 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| BMT | Flags: n z | | | | | | | | | Bytes |
|  | |  | |  | Addr12 | | Rb | 6642h | BMS zp,Rb | 3 |
|  |  | | Addr32 | | | | | 6E42h | BMS abs | 5 |
|  | Addr32 | | | | | Rb | 0 | 7E42h | BMS abs,Rb | 6 |

X index register short-form instructions.

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LDX | Flags: n z | | | | | | | | | Bytes | Cyc |
|  | |  | Immediate32 | | | | | A2h | LDX #i32 | 5 | 2 |
|  | |  | | | Immediate16 | | | B2h | LDX #i16 | 3 | 2 |
|  | |  | | | | Immediate8 | | A6h | LDX #i8 | 2 | 2 |
|  | |  | |  | Addr12 | | Rb | B6h | LDX zp,Rb | 3 |  |
|  |  | | Addr32 | | | | | AEh | LDX abs | 5 |  |
|  | Addr32 | | | | | Rb | 0 | BEh | LDX abs,Rb | 6 |  |
| STX | Flags: | | | | | | | | | Bytes |  |
|  | |  | |  | Addr12 | | Rb | 96h | STX zp,Rb | 3 |  |
|  |  | | Addr32 | | | | | 8Eh | STX abs | 5 |  |
| CPX | Flags: c n z | | | | | | | | | Bytes |  |
|  | |  | Immediate32 | | | | | E0h | CPX #i32 | 5 |  |
|  | |  | |  | Addr12 | | Rb | E4h | CPX zp,Rb | 3 |  |
|  |  | | Addr32 | | | | | ECh | CPX abs | 5 |  |
| INX | Flags: n z | | | | | | | E8h | INX | 1 | 2 |
| DEX | Flags: n z | | | | | | | CAh | DEX | 1 | 2 |
| PHX | Flags: | | | | | | | DAh | PHX | 1 |  |
| PLX | Flags: | | | | | | | FAh | PLX | 1 |  |

Y index register short-form instructions.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LDY | Flags: n z | | | | | | | | | Bytes |
|  | |  | Immediate32 | | | | | A0h | LDY #i32 | 5 |
|  | |  | |  | Addr12 | | Rb | B4h | LDY zp,Rb | 3 |
|  |  | | Addr32 | | | | | ACh | LDY abs | 5 |
|  | Addr32 | | | | | Rb | 0 | BCh | LDY abs,Rb | 6 |
| STY | Flags: | | | | | | | | | Bytes |
|  | |  | |  | Addr12 | | Rb | 94h | STY zp,Rb | 3 |
|  |  | | Addr32 | | | | | 8Ch | STY abs | 5 |
| CPY | Flags: c n z | | | | | | | | | Bytes |
|  | |  | Immediate32 | | | | | C0h | CPY #i32 | 5 |
|  | |  | |  | Addr12 | | Rb | C4h | CPY zp,Rb | 3 |
|  |  | | Addr32 | | | | | CCh | CPY abs | 5 |
| INY | Flags: n z | | | | | | | C8h | INY | 1 |
| DEY | Flags: n z | | | | | | | 88h | DEY | 1 |
| PHY | Flags: | | | | | | | 5Ah | PHY | 1 |
| PLY | Flags: | | | | | | | 7Ah | PLY | 1 |

## Flow Control

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| JMP | Flags: | | | | | | | | Bytes | Cyc |
|  | |  | Address32 | | | | 5Ch | JMP abs | 5 | 2 |
|  | |  | | Address16 | | | 4Ch | JMP abs | 3 | 2 |
|  | |  | Address32 | | | | 6Ch | JMP (abs) | 5 |  |
|  | |  | Address32 | | | | 7Ch | JMP (abs,x) | 5 |  |
|  | |  |  | | 0 | Ra | D2h | JMP (Rn) | 2 | 2 |
| JSR | Flags: | | | | | | | | Bytes |  |
|  | |  | Address32 | | | | 22h | JSR abs | 5 |  |
|  | |  | | Address16 | | | 20h | JSR abs | 3 |  |
|  | |  | Address32 | | | | FCh | JSR (abs,x) | 5 |  |
|  | |  |  | | 0 | Ra | C2h | JSR (Rn) | 2 |  |
| RTS | Flags: | | | | | | 60h | RTS | 1 |  |
| RTI | Flags: z n c v b d i | | | | | | 40h | RTI | 1 |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| BRA | Flags: | | | Disp8 | 80h | BRA disp | 2 | 2 |
| BEQ | Flags: | | | Disp8 | F0h | BEQ disp | 2 | 2 |
| BNE | Flags: | | | Disp8 | D0h | BNE disp | 2 | 2 |
| BPL | Flags: | | | Disp8 | 10h | BPL disp | 2 | 2 |
| BMI | Flags: | | | Disp8 | 30h | BMI disp | 2 | 2 |
| BVS | Flags: | | | Disp8 | 70h | BVS disp | 2 | 2 |
| BVC | Flags: | | | Disp8 | 50h | BVC disp | 2 | 2 |
| BCS | Flags: | | | Disp8 | B0h | BCS disp | 2 | 2 |
| BCC | Flags: | | | Disp8 | 90h | BCC disp | 2 | 2 |
| BHI | Flags: | | | Disp8 | 13h | BHI disp | 2 | 2 |
| BLS | Flags: | | | Disp8 | 33h | BLS disp | 2 | 2 |
| BLT | Flags: | | | Disp8 | B3h | BLT disp | 2 | 2 |
| BLE | Flags: | | | Disp8 | F3h | BLE disp | 2 | 2 |
| BGT | Flags: | | | Disp8 | D3h | BGT disp | 2 | 2 |
| BGE | Flags: | | | Disp8 | 93h | BGE disp | 2 | 2 |
| BEQ | Flags: | Disp16 | | 01h | F0h | BEQ disp | 4 | 2 |
| BNE | Flags: | Disp16 | | 01h | D0h | BNE disp | 4 | 2 |
| BPL | Flags: | Disp16 | | 01h | 10h | BPL disp | 4 | 2 |
| BMI | Flags: | Disp16 | | 01h | 30h | BMI disp | 4 | 2 |
| BVS | Flags: | Disp16 | | 01h | 70h | BVS disp | 4 | 2 |
| BVC | Flags: | Disp16 | | 01h | 50h | BVC disp | 4 | 2 |
| BCS | Flags: | Disp16 | | 01h | B0h | BCS disp | 4 | 2 |
| BCC | Flags: | Disp16 | | 01h | 90h | BCC disp | 4 | 2 |
| BRL | Flags: | | Disp16 | | 82h | BRL disp | 3 | 2 |

The range of branches is extended to 16 bits when the displacement is specified as 01h.

In 32 bit mode branch displacements are relative to the address of the branch instruction. This differs from eight bit mode where branch displacements are relative to the next instruction. In 32 bit mode a branch to self instruction, displacement = zero, triggers the SLEEP interrupt.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| BSR |  | Disp16 | 62h | BSR disp | 3 |  |
| BRK | Flags: b | | 00h | BRK | 1 |  |
| NOP | Flags: | | EAh | NOP | 1 | 2 |
| WAI | Flags: | | CBh | WAI | 1 | 2+ |
| STP | Flags: | | DBh | STP | 1 | 2 |

## Stack push and pop operations.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PHP | Flags: | | | 08h | PHP | 1 |
| PHA | Flags: | | | 48h | PHA | 1 |
| PHX | Flags: | | | DAh | PHX | 1 |
| PHY | Flags: | | | 5Ah | PHY | 1 |
| PUSH | Flags: | ~4 | Ra | 0Bh | PUSH Ra | 2 |
| PUSHA | Flags: | 0Bh | | 42h | PUSHA | 2 |
| PLP | Flags: z c v n i b d | | | 28h | PLP | 1 |
| PLA | Flags: | | | 68h | PLA | 1 |
| PLX | Flags: | | | FAh | PLX | 1 |
| PLY | Flags: | | | 7Ah | PLY | 1 |
| POP | Flags: | Rt | ~4 | 2Bh | POP Rt | 2 |
| POPA | Flags: | 2Bh | | 42h | POP Rt | 2 |

## Status Register Operations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CLC | Flags: c | 18h | CLC | 1 | 2 |
| SEC | Flags: c | 38h | SEC | 1 | 2 |
| CLV | Flags: v | B8h | CLV | 1 | 2 |
| CLI | Flags: i | 58h | CLI | 1 | 2 |
| SEI | Flags: i | 78h | SEI | 1 | 2 |
| CLD | Flags: d | D8h | CLD | 1 | 2 |
| SED | Flags: d | F8h | SED | 1 | 2 |
| EMM | Flags: m | FBh | EMM | 1 | 2 |

## Register to register transfer short forms.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TAX | Flags: n z | | | | AAh | TAX | 1 | 2 |
| TXA | Flags: n z | | | | 8Ah | TXA | 1 | 2 |
| TAY | Flags: n z | | | | A8h | TAY | 1 | 2 |
| TYA | Flags: n z | | | | 98h | TYA | 1 | 2 |
| TAS | Flags: | | | | 1Bh | TAS | 1 | 2 |
| TSA | Flags: n z | | | | 3Bh | TSA | 1 | 2 |
| TYX | Flags: n z | | | | BBh | TYX | 1 | 2 |
| TXY | Flags: n z | | | | 9Bh | TXY | 1 | 2 |
| TSX | Flags: n z | | | | BAh | TSX | 1 | 2 |
| TXS | Flags: | | | | 9Ah | TXS | 1 | 2 |
| TRS | Flags: | Spr | Ra | | 8Bh | TRS Ra,spr | 2 | 2 |
| TSR | Flags: n z | Rt | | Spr | ABh | TSR spr,Rt | 2 | 2 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| EXEC | Flags: | Rb | Ra | EBh | EXEC Ra,Rb | 2 |

The EXEC instruction executes the instruction contained in the specified register pair.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ATNI | Flags: | Rb | Ra | 4Bh | ATNI Ra,Rb | 2 |

The ATNI instruction adds a 64 bit value specified in a register pair to the next instruction. The opcodes for the next instruction executed are a combination of the instruction from memory added to registers.

## String Operations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| MVN | Flags: |  |  | 44h | MVN | 1 |
| MVP | Flags: |  |  | 54h | MVP | 1 |
| STOS | Flags: |  |  | EBh | STOS | 1 |
| CMPS | Flags: c v n z | 44h | | 42h | CMPS | 2 |

MVN – moves a block of memory beginning at low addresses and incrementing addresses and decrementing the accumulator until the accumulator which contains the count is zero. The x register contains the source address, the y register the destination address. Both x and y are incremented during the move, and the accumulator is decremented.

MVP – moves a block of memory beginning at a high address and decrementing until the accumulator is zero.

STOS – stores the value contained in the .x register to a block of memory specified by the .y register. The accumulator contains the number of words to store. This instruction is useful for initializing a block of memory to a constant value.

CMPS – compares two strings located by the x and y registers until the count in the accumulator expires, or the strings are different. The flags are set based on the comparison of the last pair of words compared.

Opcode Map – 32 bit mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | -0 | -1 | -2 | -3 | -4 | -5 | -6 | -7 | -8 | -9 | -A | -B | -C | -D | -E | -F |
| 0- | BRK | OR (d,r) | RR | OR d,s | TSB d,r | OR #i8 | ASL r,r | ~ | PHP | OR #i32 | ASL acc | PUSH r | TSB abs | OR abs | ASL abs | ~ |
| 1- | BPL disp | OR (d),r | OR (r) | BHI | TRB d,r | OR d,r | ASL d,r | ~ | CLC | OR #i16 | INA | TAS | TRB abs | OR abs,r | ASL abs,r | ~ |
| 2- | JSR abs16 | AND (d,r) | JSL abs | AND d,s | ASL #i8 | AND #i8 | ROL r,r | ~ | PLP | AND #i32 | ROL acc | POP r | JSR (abs) | AND abs | ROL abs | ~ |
| 3- | BMI disp | AND (d),r | AND (r) | BLS | LSR #i8 | AND d,r | ROL d,r | ~ | SEC | AND #i16 | DEA | TSA | ~ | AND abs,r | ROL abs,r | ~ |
| 4- | RTI | EOR (d,r) | PG2 | EOR d,s | MVP | EOR #i8 | LSR r,r | ~ | PHA | EOR #i32 | LSR acc | ATNI | JMP abs16 | EOR abs | LSR abs | ~ |
| 5- | BVC disp | EOR (d),r | EOR (r) | ~ | MVN | EOR d,r | LSR d,r | ~ | CLI | EOR #i16 | PHY | CACHE | JML abs | EOR abs,r | LSR abs,r | ~ |
| 6- | RTS | ADD (d,r) | BSR | ADD d,s | STS | ADD #i8 | ROR r,r | ~ | PLA | ADD #i32 | ROR acc | RTL | JMP (abs) | ADD abs | ROR abs | ~ |
| 7- | BVS disp | ADD (d),r | ADD (r) | ~ | SB d,r | ADD d,r | ROR d,r | ~ | SEI | ADD #i16 | PLY | LD r | JMP (abs,x) | ADD abs,r | ROR abs,r | ~ |
| 8- | BRA disp | ST (d,r) | BRL disp | ST d,s | ~ | SUB sp,#i8 | ~ | ~ | DEY | SUB sp,#i32 | TXA | TRS | STY abs | ST abs | STX abs | ~ |
| 9- | BCC disp | ST (d),r | ST (r) | BGE | STY d,r | ST d,r | STX d,r | ~ | TYA | SUB sp,#i16 | TXS | TXY | SB abs | ST abs,r | SB abs,r | ~ |
| A- | LDY #i32 | ~ | LDX #i32 | ~ | ~ | LDA #i8 | LDX #i8 | ~ | TAY | LDA #i32 | TAX | TSR | LDY abs | ORB abs | LDX abs | ~ |
| B- | BCS disp | ~ | LDX #i16 | BLT | LDY d,r | ORB d,r | LDX d,r | ~ | CLV | LDA #i16 | TSX | TYX | LDY abs,r | ORB abs,r | LDX abs,r | ~ |
| C- | CPY #i32 | BAZ | JSR (r) | ~ | CPY d,r | CMP #i8 | DEC r | ~ | INY | ~ | DEX | WAI | CPY abs | ~ | DEC abs | ~ |
| D- | BNE disp | BXZ | JMP (r) | BGT | ~ |  | DEC d,r | ~ | CLD | ~ | PHX | STP | INT #i9 | INT #i9 | DEC abs,r | ~ |
| E- | CPX #i32 | SUB (d,r) | ~ | SUB d,s | CPX d,r | SUB #i8 | INC r | ~ | INX | SUB #i32 | NOP | EXEC | CPX abs | SUB abs | INC abs | ~ |
| F- | BEQ disp | SUB (d),r | SUB(r) | BLE | ~ | SUB d,r | INC d,r | ~ | SED | SUB #i16 | PLX | EMM | JSR (abs,x) | SUB abs,r | INC abs,r | ~ |

Register-Register (RR) Instructions

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 02 | ADD | SUB | ~ | AND | EOR | OR | ~ | ~ | MUL | MULS | DIV | DIVS | MOD | MODS | ASL | LSR |

Opcode Map – 32 bit mode – Page Two (PG2 prefix) Instructions

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | -0 | -1 | -2 | -3 | -4 | -5 | -6 | -7 | -8 | -9 | -A | -B | -C | -D | -E | -F |
| 0- | ~ | MUL (d,r) | RR | MUL d,s |  | MUL #i8 | BMS d,r | ~ | ~ | MUL #i32 | ~ | PUSHA | ~ | MUL abs | BMS abs | ~ |
| 1- | ~ | MUL (d),r | MUL (r) | ~ |  | MUL d,r | ~ | ~ | TOFF | MUL #i16 | ~ | ~ | ~ | MUL abs,r | BMS abs,r | ~ |
| 2- | ~ | MULS (d,r) | ~ | MULS d,s |  | MULS #i8 | BMC d,r | ~ | ~ | MULS #i32 | ~ | POPA | ~ | MULS abs | BMC abs | ~ |
| 3- | ~ | MULS  (d),r | MULS (r) | ~ | ~ | MULS d,r | ~ | ~ | TON | MULS #i16 | ~ | ~ | ~ | MULS abs,r | BMC abs,r | ~ |
| 4- | ~ | DIV (d,r) | ~ | DIV d,s | CMPS | DIV #i8 | BMF d,r | ~ | ~ | DIV #i32 | ~ | ~ | ~ | DIV abs | BMF abs | ~ |
| 5- | ~ | DIV (d),r | DIV (r) | ~ | ~ | DIV d,r | ~ | ~ | hoff | DIV #i16 | ~ | ~ | ~ | DIV abs,r | BMF abs,x | ~ |
| 6- | ~ | DIVS (d,r) | ~ | DIVS d,s | ~ | DIVS #i8 | BMT d,r | ~ | ~ | DIVS #i32 | ~ | ~ | ~ | DIVS abs | BMT abs | ~ |
| 7- | ~ | DIVS (d),r | DIVS (r) | ~ | ~ | DIVS d,r | ~ | ~ | ~ | DIVS #i16 | ~ | ~ | ~ | DIVS abs,r | BMT abs,r | ~ |
| 8- | ~ | MOD (d,r) | ~ | MOD d,s | ~ | MOD #i8 | ~ | ~ | ~ | MOD #i32 | ~ | ~ | ~ | MOD abs | ~ | ~ |
| 9- | ~ | MOD (d),r | MOD (r) | ~ | ~ | MOD d,r | ~ | ~ | ~ | MOD #i16 | ~ | ~ | ~ | MOD abs,r | ~ | ~ |
| A- | ~ | MODS (d,r) | ~ | MODS d,s | ~ | MODS #i8 | ~ | ~ | ~ | MODS #i32 | ~ | ~ | ~ | MODS abs | ~ | ~ |
| B- | ~ | MODS (D),r | MODS (r) | ~ | ~ | MODS d,r | ~ | ~ | ~ | MODS #i16 | ~ | ~ | ~ | MODS abs,r | ~ | ~ |
| C- | ~ | LEA (d,r) | ~ | LEA d,s | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | LEA abs | ~ | ~ |
| D- | ~ | LEA (d),r | LEA (r) | ~ | ~ | LEA d,r | ~ | ~ | ~ | ~ | ~ | ~ | ~ | LEA abs,r | ~ | ~ |
| E- | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ |
| F- | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ | ~ |

Register-Register (RR) Instructions

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 4202 |  | DIF | ~ | SGN |  |  | ~ | ~ | SQRT |  |  |  |  |  |  |  |

Opcode Map – 8 bit mode W65C02 compatible

|  |  |
| --- | --- |
|  | = Enhanced instructions not found on the 65C02 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | -0 | -1 | -2 | -3 | -4 | -5 | -6 | -7 | -8 | -9 | -A | -B | -C | -D | -E | -F |
| 0- | BRK | ORA (d,x) | ~ | ~ | TSB d,r | ORA d | ASL d | ~ | PHP | OR #i8 | ASL acc | ~ | TSB abs | ORA abs | ASL abs | ~ |
| 1- | BPL disp | ORA (d),y | ORA (d) | ~ | TRB d,r | OR d,x | ASL d,x | ~ | CLC | OR abs,y | INA | TAS | TRB abs | ORA abs,x | ASL abs,x | ~ |
| 2- | JSR abs | AND (d,x) | JSL abs32 | ~ | BIT d | AND d | ROL d | ~ | PLP | AND #i8 | ROL acc | ~ | BIT abs | AND abs | ROL abs | ~ |
| 3- | BMI disp | AND (d),y | AND (d) | ~ | BIT d,x | AND d,x | ROL d,x | ~ | SEC | AND abs,y | DEA | TSA | BIT abs,x | AND abs,x | ROL abs,x | ~ |
| 4- | RTI | EOR (d,x) | ~ | ~ | ~ | EOR d | LSR d | ~ | PHA | EOR #i8 | LSR acc | ~ | JMP abs | EOR abs | LSR abs | ~ |
| 5- | BVC disp | EOR (d),y | EOR (d) | ~ | ~ | EOR d,x | LSR d,x | ~ | CLI | EOR abs,y | PHY | ~ | JML abs32 | EOR abs,x | LSR abs,x | ~ |
| 6- | RTS | ADC (d,x) | ~ | ~ | STZ d | ADC d | ROR d | ~ | PLA | ADC #i8 | ROR acc | RTL | JMP (abs) | ADC abs | ROR abs | ~ |
| 7- | BVS disp | ADC (d),y | ADC (d) | ~ | STZ d,x | ADC d,x | ROR d,x | ~ | SEI | ADC abs,y | PLY | ~ | JMP (abs,x) | ADC abs,x | ROR abs,x | ~ |
| 8- | BRA disp | STA (d,x) | BRL disp | ~ | STY d | STA d | STX d | ~ | DEY | BIT # | TXA | ~ | STY abs | STA abs | STX abs | ~ |
| 9- | BCC disp | STA (d),y | STA (d) | ~ | STY d,x | STA d,x | STX d,y | ~ | TYA | STA abs,y | TXS | TXY | STZ abs | STA abs,x | STZ abs,x | ~ |
| A- | LDY #i8 | LDA (d,x) | LDX #i8 | ~ | LDY d | LDA d | LDX d | ~ | TAY | LDA #i8 | TAX | ~ | LDY abs | LDA abs | LDX abs | ~ |
| B- | BCS disp | LDA (d),y | LDA (d) | ~ | LDY d,x | LDA d,x | LDX d,y | ~ | CLV | LDA abs,y | TSX | TYX | LDY abs,x | LDA abs,x | LDX abs,x | ~ |
| C- | CPY #i8 | CMP (d,x) | ~ | ~ | CPY d | CMP d | DEC d | ~ | INY | CMP #i8 | DEX | WAI | CPY abs | CMP abs | DEC abs | ~ |
| D- | BNE disp | CMP (d),y | CMP (d) | ~ | ~ | CMP d,x | DEC d,r | ~ | CLD | CMP abs,y | PHX | STP | ~ | CMP abs,x | DEC abs,x | ~ |
| E- | CPX #i8 | SBC(d,x) | ~ | ~ | CPX d | SUB d | INC d | ~ | INX | SBC #i8 | NOP | ~ | CPX abs | SBC abs | INC abs | ~ |
| F- | BEQ disp | SBC (d),y | SBC(r) | ~ | ~ | SUB d,x | INC d,r | ~ | SED | SBC abs,y | PLX | NAT | JSR (abs,x) | SBC abs,x | INC abs,x | ~ |